# IWF Conversion Tool

This tool converts IWF config commands from one hardware flavor to another.

Supports LTE UL/DL, WCDMA ingress/egress, and multiple hardware types like `asim`, `asib`, `asil`, etc.

## Usage


1. Modify `user\_inputs.py` to set your `from\_hardware` and `to\_hardware`.

2. Place the old config in the path defined.

3. Run `iwfChange.py`.

## Output

Generates a translated config file ready for use on the new hardware setup.



A screenshot of a computer program

AI-generated content may be incorrect.

A screenshot of a computer

AI-generated content may be incorrect.